Received 5056769 / 24bit Protocol: 1

Received 5056771 / 24bit Protocol: 1

Received 5056772 / 24bit Protocol: 1

Received 5056774 / 24bit Protocol: 1

Received 5056775 / 24bit Protocol: 1

Received 5056777 / 24bit Protocol: 1

Received 5056778 / 24bit Protocol: 1

Received 5056779 / 24bit Protocol: 1

Received 5056780 / 24bit Protocol: 1

Received 5056784 / 24bit Protocol: 1

Received 5056785 / 24bit Protocol: 1

Received 5056786 / 24bit Protocol: 1

Received 5056787 / 24bit Protocol: 1

Received 5056788 / 24bit Protocol: 1

Received 5056789 / 24bit Protocol: 1

[

/\*OFF:\*/

int lightOff = 5056769;

/\*ON:\*/

int lightOn = 5056771;

/\*Dimmer:\*/

int dim = 5056772;

/\*Brighter:\*/

int bright = 5056774;

/\*Prev Color:\*/

int prevColor = 5056775;

/\*Next Color:\*/

int nextColor = 5056777;

/\*Slow Cycle:\*/

int slowCycle = 5056778;

/\*Mode Switch:\*/

int modeSwitch = 5056779;

/\*Fast Cycle:\*/

int fastCycle = 5056780;

/\*RGB White:\*/

int rgbWhite = 5056784;

/\*True White:\*/

int trueWhite = 5056785;

/\*Warm White:\*/

int warmWhite = 5056786;

/\*Red:\*/

int red = 5056787;

/\*Blue:\*/

int blue = 5056788;

/\*Green:\*/

int green = 5056789;

/\*

\* Cut-and-paste into the area above.

\*/

]

Decimal: 5056772 (24Bit) Binary: 010011010010100100000100 Tri-State: not applicable PulseLength: 394 microseconds Protocol: 1

Raw data: 12244,376,1264,1240,488,376,1264,376,1264,1212,500,1212,512,356,1284,1208,520,364,1276,364,1276,1220,500,368,1272,1204,512,360,1284,360,1284,1220,512,208,676,252,684,216,692,208,1276,364,680,228,692,244,672,224,744,

Decimal: 5056771 (24Bit) Binary: 010011010010100100000011 Tri-State: not applicable PulseLength: 394 microseconds Protocol: 1

Raw data: 12228,380,1264,1236,488,380,1260,372,1264,1228,496,1228,492,372,1264,1224,508,364,1272,372,1276,1220,496,364,1272,1224,500,368,1268,372,1272,1220,500,44,1684,144,1732,164,1712,180,700,440,488,332,800,40,748,216,780,

Decimal: 5056772 (24Bit) Binary: 010011010010100100000100 Tri-State: not applicable PulseLength: 394 microseconds Protocol: 1

Raw data: 12232,376,1264,1228,492,376,1264,380,1260,1232,488,1228,492,376,1268,1224,500,372,1264,372,1268,1228,492,376,1268,1224,492,372,1268,372,1272,1224,500,372,1268,368,1272,372,1268,368,1268,372,1268,1224,496,372,1276,368,1264,

Decimal: 5056774 (24Bit) Binary: 010011010010100100000110 Tri-State: not applicable PulseLength: 394 microseconds Protocol: 1

Raw data: 12224,380,1256,1236,496,368,1264,380,1256,1232,488,1228,492,376,1264,1228,496,380,1268,368,1268,1228,492,372,1272,1220,492,372,1268,372,1268,1228,500,372,1268,372,1264,376,1264,360,548,344,668,180,648,320,588,292,240,

Decimal: 5056775 (24Bit) Binary: 010011010010100100000111 Tri-State: not applicable PulseLength: 394 microseconds Protocol: 1

Raw data: 12228,380,1260,1232,488,376,1260,380,1264,1228,492,1228,488,376,1272,1220,500,372,1268,372,1268,1224,496,368,1272,1224,496,368,1268,376,1268,1224,500,368,1276,368,788,60,3360,16,1772,36,580,312,640,252,684,580,332,

Decimal: 5056777 (24Bit) Binary: 010011010010100100001001 Tri-State: not applicable PulseLength: 394 microseconds Protocol: 1

Raw data: 12224,384,1256,1228,484,384,1260,380,1256,1228,492,1228,492,372,1276,1220,496,376,1260,372,1272,1224,492,372,1272,1220,492,372,1264,376,1268,1224,500,368,1268,368,1276,364,1272,372,1268,1220,496,368,1272,372,1268,1220,500,

Decimal: 5056778 (24Bit) Binary: 010011010010100100001010 Tri-State: not applicable PulseLength: 394 microseconds Protocol: 1

Raw data: 12220,380,1264,1228,488,376,1260,380,1264,1228,488,1228,492,376,1268,1224,496,376,1264,376,1268,1220,496,372,1268,1224,492,372,1268,376,1264,1228,500,372,1264,372,1268,372,1268,372,1268,1224,500,184,868,104,652,344,600,

Decimal: 5056779 (24Bit) Binary: 010011010010100100001011 Tri-State: not applicable PulseLength: 394 microseconds Protocol: 1

Raw data: 12228,384,1260,1232,492,372,1264,372,1264,1212,512,1204,508,356,1284,1220,504,368,1272,360,1276,1224,492,372,1268,1216,504,360,1276,368,124,808,120,752,140,360,1276,252,648,284,492,380,2432,148,668,536,356,628,256,

Decimal: 5056780 (24Bit) Binary: 010011010010100100001100 Tri-State: not applicable PulseLength: 393 microseconds Protocol: 1

Raw data: 12228,380,1256,1220,504,364,1276,372,1264,1216,504,1212,508,360,1276,1224,504,364,1276,356,1276,1216,504,364,1284,1208,500,364,1280,364,1276,1216,508,364,672,276,932,52,56,40,616,432,588,288,616,260,556,496,416,

Decimal: 5056784 (24Bit) Binary: 010011010010100100010000 Tri-State: not applicable PulseLength: 393 microseconds Protocol: 1

Raw data: 12216,376,1264,1228,488,380,1260,380,1264,1228,488,1228,496,372,1260,1224,500,372,1272,368,1272,1220,492,376,1268,1224,492,372,1268,372,1268,1220,500,372,1276,368,1268,368,1272,1220,496,368,1272,368,1268,372,1272,368,1268,

Decimal: 5056785 (24Bit) Binary: 010011010010100100010001 Tri-State: not applicable PulseLength: 393 microseconds Protocol: 1

Raw data: 12220,380,1256,1232,488,376,1268,376,1264,1224,492,1224,492,376,1268,1224,504,368,1264,368,1268,1224,496,372,1272,1220,496,368,1268,372,1268,1224,504,364,1268,372,1264,372,1272,1220,496,368,1276,364,1276,364,1268,1224,496,

Decimal: 5056786 (24Bit) Binary: 010011010010100100010010 Tri-State: not applicable PulseLength: 393 microseconds Protocol: 1

Raw data: 12220,372,1260,1232,492,372,1264,380,1264,1228,488,1228,492,372,1272,1224,500,372,1260,376,1264,1220,500,368,1276,1216,492,372,1272,372,1268,1220,496,376,1264,372,1272,368,1272,1220,496,372,1268,368,1268,1220,500,364,1272,

Decimal: 5056787 (24Bit) Binary: 010011010010100100010011 Tri-State: not applicable PulseLength: 394 microseconds Protocol: 1

Raw data: 12220,384,1260,1224,496,372,1260,376,1264,1228,492,1224,492,376,1264,1224,504,368,1276,364,1268,1224,492,372,1268,1224,500,368,1272,364,1276,1216,500,368,1276,364,1272,368,1276,1216,496,464,428,544,236,48,44,604,252,

Decimal: 5056788 (24Bit) Binary: 010011010010100100010100 Tri-State: not applicable PulseLength: 394 microseconds Protocol: 1

Raw data: 12252,356,1276,1216,508,364,1276,360,1276,1208,508,1212,504,368,1300,1184,532,332,1284,352,1296,1212,536,324,1292,1192,508,360,1296,352,1300,1184,512,352,1276,356,1292,364,1300,1192,512,340,1292,316,620,308,592,348,664,

Decimal: 5056789 (24Bit) Binary: 010011010010100100010101 Tri-State: not applicable PulseLength: 394 microseconds Protocol: 1

Raw data: 12236,368,1268,1228,492,372,1276,368,1268,1220,500,1220,496,372,1268,1220,500,372,1268,368,1276,1224,496,368,1276,1216,496,372,1268,368,1272,1220,500,372,1268,368,1276,364,1284,1208,500,372,1268,1216,500,368,1272,1220,500,